**********************  IBM  *******************************************
* :nick.XR06100A   :sec.IBM                           :disk.OS2CSD
* :title.OS/2 V2.0 ServicePak XR06100 U.S.(3.50") media
* :version.2.0     :date.93/08/30   :summary.AVAIL    :support.N
* :oname.OS2CSD Disk                :onode.KGNVMZ     :ouser.PRODCTR
* :aname.OS/2 Local Control Group   :anode.AUSVM8     :auser.AUSLCG
* :ops.OS/2 V2.0
* :abs.This ServicePak contains the fixes for OS/2 version 2.00, also
* included are Display Drivers, and Printer Drivers. If you experience
* problems with the ServicePak contact your local support center.
* 5.25" media is not available.
*************************************************************************
* Diskettes can be created using the LOADDSKF utility, this utility
* may be obtained from the /ps/tools directory.                     
* There are 17 images included in this package.
*************************************************************************
* The diskettes contained in this package may be distributed to
* IBM customers who are already licensed owners of OS/2 Version 2.0
* by IBM marketing personnel authorized to service that customer.
************************************************************************
  XR06100  CID  *  CID (RIPL) install tips (ascii)
  XR06100  FIX  *  APARs fixed by XR06100 ServicePak (ascii)
  XR06100  AVL  *  Info regarding ServicePak XR06100 (ascii)
  XR06100A LAB  *  Diskette Labels for ServicePak (ascii)
  06100B1  DSK  *  Disk 1 of 12, ServicePak Diskette  CRC=X'8E27 ' (binary)
  06100B2  DSK  *  Disk 2 of 12, ServicePak Diskette  CRC=X'66A3 ' (binary)
  06100B3  DSK  *  Disk 3 of 12, ServicePak Diskette  CRC=X'B402 ' (binary)
  06100B4  DSK  *  Disk 4 of 12, ServicePak Diskette  CRC=X'68F0 ' (binary)
  06100B5  DSK  *  Disk 5 of 12, ServicePak Diskette  CRC=X'881B ' (binary)
  06100B6  DSK  *  Disk 6 of 12, ServicePak Diskette  CRC=X'9331 ' (binary)
  06100B7  DSK  *  Disk 7 of 12, ServicePak Diskette  CRC=X'820E ' (binary)
  06100B8  DSK  *  Disk 8 of 12, ServicePak Diskette  CRC=X'00D7 ' (binary)
  06100B9  DSK  *  Disk 9 of 12, ServicePak Diskette  CRC=X'EDA1 ' (binary)
  06100B10 DSK  *  Disk 10 of 12, ServicePak Diskette CRC=X'6E6B ' (binary)
  06100B11 DSK  *  Disk 11 of 12, ServicePak Diskette CRC=X'D68E ' (binary)
  06100B12 DSK  *  Disk 12 of 12, ServicePak Diskette CRC=X'4E33 ' (binary)
  06100B13 DSK  *  Disk 01 of 02, Display Driver Disk CRC=X'C152 ' (binary)
  06100B14 DSK  *  Disk 02 of 02, Display Driver Disk CRC=X'C061 ' (binary)
  06100B15 DSK  *  Disk 01 of 03, Printer Driver Disk CRC=X'E3D2 ' (binary)
  06100B16 DSK  *  Disk 02 of 03, Printer Driver Disk CRC=X'A4B4 ' (binary)
  06100B17 DSK  *  Disk 03 of 03, Printer Driver Disk CRC=X'F189 ' (binary)
* End of package
