========== StorageAdapterDescriptor ==========
	              Version: 32
	                 Size: 32
	MaximumTransferLength: 131072 (bytes)
	 MaximumPhysicalPages: 33
	        AlignmentMask: 1 (Buffers must be aligned on WORD boundaries)
	       AdapterUsesPio: False
	     AdapterScansDown: False
	      CommandQueueing: True
	  AcceleratedTransfer: False
	              BusType: BusTypeAtapi
	      BusMajorVersion: 2
	      BusMinorVersion: 0
dwMaxTransferLength changed [131072] -> [65536]
========== IoctlScsiGetAddress ==========
	    Length: 8
	PortNumber: 0
	    PathId: 0
	  TargetId: 0
	       Lun: 0
========== InquiryData ==========
	          DeviceType: ReadOnlyDirectAccessDevice (CD/DVD etc)
	 DeviceTypeQualifier: Active
	  DeviceTypeModifier: 0
	      RemovableMedia: Yes
	            Versions: 0
	  ResponseDataFormat: 2
	           HiSupport: Yes
	             NormACA: Yes
	       TerminateTask: No
	                AERC: No
	    AdditionalLength: 91
	       MediumChanger: No
	           MultiPort: No
	   EnclosureServices: No
	           SoftReset: No
	        CommandQueue: No
	      LinkedCommands: No
	  RelativeAddressing: No
	            VendorId: PLEXTOR 
	           ProductId: DVDR   PX-755A  
	ProductRevisionLevel: 1.08
	      VendorSpecific: 08/18/07  15:10     
========== EEPROM ==========
	      Signature: a3 03
	       VendorId: PLEXTOR 
	      ProductId: DVDR   PX-755A  
	   SerialNumber: 110358
	   Unknown[031]: ff 23 00 00 06 33 03 01 13 6c 
	            TLA: 0002
	   Unknown[045]: ff ff ff 00 05 ff 00 ff ff ff ff ff ff fa ff ff fb f1 ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 00 75 12 1f 02 f8 0d 44 56 fb ff 82 67 ff 02 fc 02 0b 70 0e 00 39 bb 40 ba 51 f4 5b 
	   Unknown[108]: 18 00 de ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 10 10 ff ff ff ff ff ff ff a6 ff ff ff ff 00 70 0f 1e f9 04 11 66 35 02 02 02 74 00 00 0a 00 05 05 00 fa fc 00 00 44 33 10 0f ff ff ff ff ff 35 c9 1c dd ff 03 00 00 00 00 ff ff ff ff ff ee ff fe f0 01 f5 06 06 04 5f 00 45 02 97 04 87 0a 60 0d 10 21 b6 2e fd 33 85 46 09 ff ff ff ff 26 f2 22 e1 1e 32 06 fe 00 01 e5 e5 ff ff 1b 41 01 3f 00 00 01 74 01 2d 01 db 01 82 25 f4 80 59 
	    Silent Mode: Enabled
		       Access Time: Fast
		    Max Read Speed: 40x
		           Unknown: 16x
		   Max Write Speed: 8x
		           Unknown: 20x
		           Unknown: 01
		  Tray Speed Eject: d0 (Low d0 - 80 High)
		Tray Speed Loading: 2f (Low 2f - 7f High)
	        SecuRec: ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 
	      SpeedRead: Enable
	        Unknown: ff
	  Spindown Time: 2 minites
	Disc load count: 1325
	   CD read time: 90:03:52
	  CD write time: 09:47:41
	  DVD read time: 65:42:51
	 DVD write time: 10:51:26
	   Unknown[050]: 00 00 00 00 ff 0c d8 aa 02 8d 73 03 04 04 00 00 00 40 00 ff ff ff ff ff ff ff ff ff ff ff 00 00 00 00 00 00 00 00 ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 02 03 04 
	Change BookType: Disable
	  Auto Strategy: Auto Selection
	   Unknown[117]: ff ff ff ff ff ff ff ff ff ff ff ff ff 00 00 ff ff ff ff ff ff ff ff ff ff ff ff 01 02 02 0b 0c 0c ff ff ff 0d 02 00 ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 00 01 00 01 00 00 00 01 00 33 00 00 ff ff ff ff ff 23 02 ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 0a 0c ff ff ff ff ff ff ff ff b2 
	            Sum: 39 (SpeedRead: f0 + Spindown Time: 0b + BookType: ff + Auto Strategy: 0f + Others)
	   Unknown[000]: ff 03 00 ff ff ff ff ff 0d ad 5e 42 00 88 ff ff 1f f7 fe 0a ff 00 0a ff ff ff 4f 4e 4f 18 ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 80 fd 00 2c ff ff ff ff ff ff 01 ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 00 00 00 95 ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff 35 30 31 38 4b 34 2d 35 36 44 53 31 30 4b 20 30 20 46 44 46 42 4a 31 38 41 33 32 ff ff ff ff ff 46 43 35 46 55 55 ff 04 08 01 00 f1 00 ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff cb 43 
	   Unknown[000]: ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff ff fd 02 
========== GetConfiguration ==========
	    DataLength: 256
	CurrentProfile: CD-ROM
	FeatureProfileList
		DVD+R DL
		DVD+R
		DVD+RW
		DVD-R Layer Jump
		DVD-R DL
		DVD-RW Sequential
		DVD-RW
		DVD-R
		DVD-ROM
		CD-RW
		CD-R
		CD-ROM
	FeatureCore
		PhysicalInterface: Serial ATAPI
		  DeviceBusyEvent: No
		         INQUIRY2: No
	FeatureMorphing
		Asynchronous: No
		     OCEvent: No
	FeatureRemovableMedium
		        Lockable: Yes
		DefaultToPrevent: No
		           Eject: Yes
		LoadingMechanism: Tray type loading mechanism
	FeatureRandomReadable
		        LogicalBlockSize: 2048
		                Blocking: 1
		ErrorRecoveryPagePresent: Yes
	FeatureMultiRead
		   Current: 1
		Persistent: 0
		   Version: 0
	FeatureCdRead
		          CDText: Yes
		     C2ErrorData: Yes
		DigitalAudioPlay: No
	FeaturePowerManagement
		   Current: 1
		Persistent: 1
		   Version: 0
	FeatureMicrocodeUpgrade
		M5: Yes
	FeatureTimeout
		    Group3: Yes
		UnitLength: 3332
	FeatureRealTimeStreaming
		        StreamRecording: Yes
		    WriteSpeedInGetPerf: Yes
		       WriteSpeedInMP2A: Yes
		             SetCDSpeed: Yes
		ReadBufferCapacityBlock: Yes
	FeatureLogicalUnitSerialNumber
		SerialNumber: 110358  
	VendorSpecific (FeatureCode[0xff00])
		VendorSpecificData: 01010103
	VendorSpecific (FeatureCode[0xff02])
		VendorSpecificData: 
	VendorSpecific (FeatureCode[0xff10])
		VendorSpecificData: 000a0004058302c200090004058302c2
	VendorSpecific (FeatureCode[0xff11])
		VendorSpecificData: 002b000a361a2b48207615a40cfc001b000e6162569040ec2b48207615a40cfc001a00082b48207615a40cfc001500062b48207615a400140008207615a40ad205690011000e6162569040ec2b48207615a40ad2
========== ModeParmeterHeader10 ==========
	         ModeDataLength: 58
	             MediumType: 1
	DeviceSpecificParameter: 0
	  BlockDescriptorLength: 0
========== CDVD Capabilities & Mechanism Status Page ==========
	              PageCode: 0x2a
	                 PSBit: No
	            PageLength: 50
	               CDRRead: Yes
	               CDERead: Yes
	               Method2: Yes
	            DVDROMRead: Yes
	              DVDRRead: Yes
	            DVDRAMRead: No
	              CDRWrite: Yes
	              CDEWrite: Yes
	             TestWrite: Yes
	             DVDRWrite: Yes
	           DVDRAMWrite: No
	             AudioPlay: Yes
	             Composite: Yes
	        DigitalPortOne: No
	        DigitalPortTwo: No
	            Mode2Form1: Yes
	            Mode2Form2: Yes
	          MultiSession: Yes
	    BufferUnderrunFree: Yes
	                  CDDA: Yes
	          CDDAAccurate: Yes
	           RWSupported: Yes
	       RWDeinterleaved: Yes
	            C2Pointers: Yes
	                  ISRC: Yes
	                   UPC: Yes
	    ReadBarCodeCapable: No
	                  Lock: Yes
	             LockState: No
	         PreventJumper: No
	                 Eject: Yes
	  LoadingMechanismType: tray
	        SeparateVolume: Yes
	   SeperateChannelMute: Yes
	   SupportsDiskPresent: No
	       SWSlotSelection: No
	     SideChangeCapable: No
	    RWInLeadInReadable: Yes
	      ReadSpeedMaximum: 7056KB/sec (40x)
	    NumberVolumeLevels: 256
	            BufferSize: 2048
	      ReadSpeedCurrent: 1411KB/sec (8x)
	                   BCK: No
	                   RCK: No
	                  LSBF: No
	                Length: 0
	     WriteSpeedMaximum: 1411KB/sec (8x)
	     WriteSpeedCurrent: 1411KB/sec (8x)
	CopyManagementRevision: 0
========== ReadBufferCapacity ==========
	    TotalBufferSize: 1162KByte
	AvailableBufferSize: 1162KByte
========== SetSpeed ==========
	    RequestType: CdromSetSpeed
	      ReadSpeed: 8467KB/sec
	     WriteSpeed: 308KB/sec
	RotationControl: CdromCAVRotation
========== Check main+c2+sub ==========
========== LBA[000000, 0000000]: C2 error ==========
       +0 +1 +2 +3 +4 +5 +6 +7
0000 : 00 00 00 00 00 00 00 00
0008 : 00 00 00 00 00 00 00 00
0010 : 00 00 00 00 00 00 00 00
0018 : 00 00 00 00 00 00 00 00
0020 : 00 00 00 00 00 00 00 00
0028 : 00 00 00 00 00 00 00 00
0030 : 00 00 00 00 00 00 00 00
0038 : 00 00 00 00 00 00 00 00
0040 : 00 00 00 00 00 00 00 00
0048 : 00 00 00 00 00 00 00 00
0050 : 00 00 00 00 00 00 00 00
0058 : 00 00 00 00 00 00 00 00
0060 : 00 00 00 00 00 00 00 00
0068 : 00 00 00 00 00 00 00 00
0070 : 00 00 00 00 00 00 00 00
0078 : 00 00 00 00 00 00 00 00
0080 : 00 00 00 00 00 00 00 00
0088 : 00 00 00 00 00 00 00 00
0090 : 00 00 00 00 00 00 00 00
0098 : 00 00 00 00 00 00 00 00
00A0 : 00 00 00 00 00 00 00 00
00A8 : 00 00 00 00 00 00 00 00
00B0 : 00 00 00 00 00 00 00 00
00B8 : 00 00 00 00 00 00 00 00
00C0 : 00 00 00 00 00 00 00 00
00C8 : 00 00 00 00 00 00 00 00
00D0 : 00 00 00 00 00 00 00 00
00D8 : 00 00 00 00 00 00 00 00
00E0 : 00 00 00 00 00 00 00 00
00E8 : 00 00 00 00 00 00 00 00
00F0 : 00 00 00 00 00 00 00 00
00F8 : 00 00 00 00 00 00 00 00
0100 : 00 00 00 00 00 00 00 00
0108 : 00 00 00 00 00 00 00 00
0110 : 00 00 00 00 00 00 00 00
0118 : 00 00 00 00 00 00 00 00
0120 : 00 00 00 00 00 00 80 C0
========== LBA[000000, 0000000]: Sub Channel(Raw) ==========
       +0 +1 +2 +3 +4 +5 +6 +7  +8 +9 +A +B +C +D +E +F
0000 : 80 C0 C0 80 80 80 80 C0  80 80 80 80 80 80 80 C0
0010 : 80 80 80 80 80 80 80 C0  80 80 80 80 80 80 80 80
0020 : 80 80 80 80 80 80 80 80  80 80 80 80 80 80 80 80
0030 : 80 80 80 80 80 80 80 80  80 80 80 80 80 80 80 80
0040 : 80 80 80 80 80 80 C0 80  80 80 80 80 80 80 80 80
0050 : 80 80 80 C0 80 80 80 C0  80 80 C0 C0 C0 C0 C0 C0
========== Check main+sub+c2 ==========
========== LBA[000000, 0000000]: Sub Channel(Raw) ==========
       +0 +1 +2 +3 +4 +5 +6 +7  +8 +9 +A +B +C +D +E +F
0000 : 00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00
0010 : 00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00
0020 : 00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00
0030 : 00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00
0040 : 00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00
0050 : 00 00 00 00 00 00 00 00  00 00 00 00 00 00 00 00
========== LBA[000000, 0000000]: C2 error ==========
       +0 +1 +2 +3 +4 +5 +6 +7
0000 : 00 00 00 00 00 00 00 00
0008 : 00 00 00 00 00 00 00 00
0010 : 00 00 00 00 00 00 00 00
0018 : 00 00 00 00 00 00 00 00
0020 : 00 00 00 00 00 00 00 00
0028 : 00 00 00 00 00 00 00 00
0030 : 00 00 00 00 00 00 00 00
0038 : 00 00 00 00 00 00 00 00
0040 : 00 00 00 00 00 00 00 00
0048 : 00 00 00 00 00 00 00 00
0050 : 00 00 00 00 00 00 00 00
0058 : 00 00 00 00 00 00 00 00
0060 : 00 00 00 00 00 00 00 00
0068 : 00 00 00 00 00 00 00 00
0070 : 00 00 00 00 00 00 00 00
0078 : 00 00 00 00 00 00 00 00
0080 : 00 00 00 00 00 00 00 00
0088 : 00 00 00 00 00 00 00 00
0090 : 00 00 00 00 00 00 00 00
0098 : 00 00 00 00 00 00 00 00
00A0 : 00 00 00 00 00 00 00 00
00A8 : 00 00 00 00 00 00 00 00
00B0 : 00 00 00 00 00 00 00 00
00B8 : 00 00 00 00 00 00 00 00
00C0 : 00 00 00 00 00 00 80 C0
00C8 : C0 80 80 80 80 C0 80 80
00D0 : 80 80 80 80 80 C0 80 80
00D8 : 80 80 80 80 80 C0 80 80
00E0 : 80 80 80 80 80 80 80 80
00E8 : 80 80 80 80 80 80 80 80
00F0 : 80 80 80 80 80 80 80 80
00F8 : 80 80 80 80 80 80 80 80
0100 : 80 80 80 80 80 80 80 80
0108 : 80 80 80 80 C0 80 80 80
0110 : 80 80 80 80 80 80 80 80
0118 : 80 C0 80 80 80 C0 80 80
0120 : C0 C0 C0 C0 C0 C0 00 00
	Byte order of this drive is main + c2 + sub
This drive supports [OpCode: 0xd8, SubCode: 0]
This drive supports [OpCode: 0xd8, SubCode: 1]
This drive supports [OpCode: 0xd8, SubCode: 2]
This drive supports [OpCode: 0xd8, SubCode: 8]
Checking reading lead-out -> OK
